### Capabilities

# Gear Grinding

#### ECONOMICAL SOLUTIONS FOR PRECISION GEAR GRINDING

Starting in 2007 Riverside Spline & Gear started construction of our new 10,000 sq. ft. Gear Grinding Center. Our first acquisition was the new 2007 Hofler 900 which allowed us to grind a gear as large as 39 inches.

Today we have added four more new grinders consisting of two Hofler 700, a Hofler Helix 400 and a Hofler Rapid 1500L. All five machines are equipped with on board checking and operate 23 hours a day.

Riverside is known in the industry for its quality and quick turnaround on gear grinding. This is why many other gear companies continue to use us as their gear grinding source.

EXTERNAL GEARS
Gear Diameter | 12-1500 mm | .5" to 59"
Center Distance Above Table | 360-1500 mm | 14.2" - 59"
Axial Stroke (Max) | 1500 mm | 59"
Helix Angle | +- 45°, 90° | +- 45°, 90°
Module | 1-25 mm(extendable to 34 mm) | 15DP - 1.25 DP
Profile Height | 41 mm(extendable to 60-80 mm) | 1.6"
Grinding Wheel Width | 60 mm (extendable to 90 mm) | 2.95"
Grinding Wheel Diameter | 400 mm | 15.75" to 4"
Table Load | 6000 kg | 13,227 Lbs.